Correction to Smooth Sailing Pattern – Step 2

2 a) Make the 24” and the two 14” Compass Quarter Units following the instructions from the Skinny Robin 45˚ Mariner’s Compass Book all the way to Step 28 to make your quarter units **except sew the Point 3 strip on the the opposite side of Big Pie (you will have to turn your ruler over to make the Point 3 cut)**. Clean up your blocks by trimming off protruding points around the raw block perimeter.

Make a 24” and 14” freezer paper quarter circle. Press these onto the back of the corresponding Compass Quarter Units, and press the edge around the freezer paper. Remove freezer paper and pin pressed edges.

b) Appliqué these Compass Quarter units onto the B-6 and BX-6 rectangles for the Sailboat blocks. Sew them with a straight stitch or hem stitch on your machine, or hand appliqué. c) Trim off the protruding

Point 3 fabric flush with the rectangle.